set_property SRC_FILE_INFO {cfile:D:/Documents/VivadoProjects/PipelineProcessor/PipelineProcessor.srcs/constrs_1/new/top.xdc rfile:../../../PipelineProcessor.srcs/constrs_1/new/top.xdc id:1} [current_design]
set_property src_info {type:XDC file:1 line:1 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN R4 IOSTANDARD LVCMOS33} [get_ports {hardware_clk}]
set_property src_info {type:XDC file:1 line:4 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN B22 IOSTANDARD LVCMOS33} [get_ports {hardware_reset}]
set_property src_info {type:XDC file:1 line:6 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN V2 IOSTANDARD LVCMOS33} [get_ports {clock_locked}]
set_property src_info {type:XDC file:1 line:9 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN N2 IOSTANDARD LVCMOS33} [get_ports {bcd_control[0]}]
set_property src_info {type:XDC file:1 line:11 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN P5 IOSTANDARD LVCMOS33} [get_ports {bcd_control[1]}]
set_property src_info {type:XDC file:1 line:12 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN V5 IOSTANDARD LVCMOS33} [get_ports {bcd_control[2]}]
set_property src_info {type:XDC file:1 line:13 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN U5 IOSTANDARD LVCMOS33} [get_ports {bcd_control[3]}]
set_property src_info {type:XDC file:1 line:14 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN T5 IOSTANDARD LVCMOS33} [get_ports {bcd_control[4]}]
set_property src_info {type:XDC file:1 line:15 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN P1 IOSTANDARD LVCMOS33} [get_ports {bcd_control[5]}]
set_property src_info {type:XDC file:1 line:16 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN W4 IOSTANDARD LVCMOS33} [get_ports {bcd_control[6]}]
set_property src_info {type:XDC file:1 line:17 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN V3 IOSTANDARD LVCMOS33} [get_ports {bcd_control[7]}]
set_property src_info {type:XDC file:1 line:19 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN Y3 IOSTANDARD LVCMOS33} [get_ports {bcd_control[8]}]
set_property src_info {type:XDC file:1 line:20 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN R1 IOSTANDARD LVCMOS33} [get_ports {bcd_control[9]}]
set_property src_info {type:XDC file:1 line:21 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN P2 IOSTANDARD LVCMOS33} [get_ports {bcd_control[10]}]
set_property src_info {type:XDC file:1 line:22 export:INPUT save:INPUT read:READ} [current_design]
set_property -dict {PACKAGE_PIN M2 IOSTANDARD LVCMOS33} [get_ports {bcd_control[11]}]
